Safe Output - Output Driver (High Side Switch)

Page / - last modified by Michael Kieviet on 2023/06/20 10:48

Output Driver (High Side Switch)

last modified by Michael Kieviet

on 2023/06/20 10:48

Table of Contents

https://www.infineon.com/cms/en/product/power/smart-power-switches/high-side-switches/profet-plus-24v-automotive-smart-high-side-switch/#!products

Infineon Smart High-Side Power Switch Single Channel Driver

I load : 1.5 A

Maximum supply voltage: 65V

BTT6200-1ENA

Aus <https://www.infineon.com/dgdl/Infineon-BTT6200-1ENA-DS-v01_00-EN.pdf?fileId=5546d462636cc8fb01645f3a31f312e9>

ST

IPS160H, IPS 161H

I load 2,5A

Max. operating Voltage 60V

Designed to meet IEC61131-2

https://www.st.com/en/applications/factory-automation/industrial-safety.html#documentation